Applicability of Abstraction and Control of Traffic Engineered Networks (ACTN) to Packet Optical Integration (POI)

draft-peru-teas-actn-poi-applicability-06

Status of this Memo

This Internet-Draft is submitted in full conformance with the provisions of BCP 78 and BCP 79.

Internet-Drafts are working documents of the Internet Engineering Task Force (IETF), its areas, and its working groups. Note that other groups may also distribute working documents as Internet-Drafts.

Internet-Drafts are draft documents valid for a maximum of six months and may be updated, replaced, or obsoleted by other documents at any time. It is inappropriate to use Internet-Drafts as reference material or to cite them other than as "work in progress."

The list of current Internet-Drafts can be accessed at http://www.ietf.org/ietf/1id-abstracts.txt

The list of Internet-Draft Shadow Directories can be accessed at http://www.ietf.org/shadow.html

This Internet-Draft will expire on February 18, 2020.

Copyright Notice

Copyright (c) 2020 IETF Trust and the persons identified as the document authors. All rights reserved.

This document is subject to BCP 78 and the IETF Trust’s Legal Provisions Relating to IETF Documents (http://trustee.ietf.org/license-info) in effect on the date of publication of this document. Please review these documents carefully, as they describe your rights and restrictions with respect to this document. Code Components extracted from this document must include Simplified BSD License text as described in Section 4.e of the Trust Legal Provisions and are provided without warranty as described in the Simplified BSD License.

Abstract

This document considers the applicability of Abstraction and Control of TE Networks (ACTN) architecture to Packet Optical Integration (POI)in the context of IP/MPLS and Optical internetworking, identifying the YANG data models being defined by the IETF to support this deployment architecture as well as specific scenarios relevant for Service Providers.

Existing IETF protocols and data models are identified for each multi-layer (packet over optical) scenario with particular focus on the MPI (Multi-Domain Service Coordinator to Provisioning Network Controllers Interface)in the ACTN architecture.

Table of Contents

[1. Introduction 3](#_Toc42249109)

[2. Reference architecture and network scenario 4](#_Toc42249110)

[2.1. Generic Assumptions 7](#_Toc42249111)

[2.2. L2/L3VPN/VN Service Request by the Customer 7](#_Toc42249112)

[2.3. Service and Network Orchestration 9](#_Toc42249113)

[2.4. IP/MPLS Domain Controller and NE Functions 12](#_Toc42249114)

[2.5. Optical Domain Controller and NE Functions 15](#_Toc42249122)

[3. Multi-layer and multi-domain services scenarios 17](#_Toc42249123)

[3.1. Scenario 1: network and service topology discovery 17](#_Toc42249124)

[3.1.1. Common YANG models used at MPIs 18](#_Toc42249126)

[3.1.2. Required YANG models at the optical MPIs 19](#_Toc42249127)

[3.1.3. Required YANG models at the Packet MPIs 20](#_Toc42249128)

[3.1.4. Inter-domain link discovery 21](#_Toc42249129)

[3.2. L2VPN/L3VPN establishment 22](#_Toc42249130)

[4. Security Considerations 22](#_Toc42249131)

[5. Operational Considerations 22](#_Toc42249132)

[6. IANA Considerations 22](#_Toc42249133)

[7. References 22](#_Toc42249134)

[7.1. Normative References 22](#_Toc42249135)

[7.2. Informative References 23](#_Toc42249136)

[8. Acknowledgments 25](#_Toc42249137)

[Appendix A. Multi-layer and multi-domain resiliency 26](#_Toc42249138)

[A.1. Maintenance Window 26](#_Toc42249139)

[A.2. Router port failure 26](#_Toc42249140)

[Authors’ Addresses 26](#_Toc42249141)

# Introduction

The full automation of the management and control of Service Providers transport networks (IP/MPLS, Optical and also Microwave) is key for achieving the new challenges coming now with 5G as well as with the increased demand in terms of business agility and mobility in a digital world. ACTN architecture, by abstracting the network complexity from Optical and IP/MPLS networks towards MDSC and then from MDSC towards OSS/BSS or Orchestration layer through the use of standard interfaces and data models, is allowing a wide range of transport connectivity services that can be requested by the upper layers fulfilling almost any kind of service level requirements from a network perspective (e.g. physical diversity, latency, bandwidth, topology etc.)

Packet Optical Integration (POI) is an advanced use case of traffic engineering. In wide area networks, a packet network based on the Internet Protocol (IP) and possibly Multiprotocol Label Switching (MPLS) is typically realized on top of an optical transport network that uses Dense Wavelength Division Multiplexing (DWDM)(and optionally an Optical Transport Network (OTN)layer). In many existing network deployments, the packet and the optical networks are engineered and operated independently of each other. There are technical differences between the technologies (e.g., routers vs. optical switches) and the corresponding network engineering and planning methods (e.g., inter-domain peering optimization in IP vs. dealing with physical impairments in DWDM, or very different time scales). In addition, customers needs can be different between a packet and an optical network, and it is not uncommon to use different vendors in both domains. Last but not least, state-of-the-art packet and optical networks use sophisticated but complex technologies, and for a network engineer it may not be trivial to be a full expert in both areas. As a result, packet and optical networks are often operated in technical and organizational silos.

This separation is inefficient for many reasons. Both capital expenditure (CAPEX) and operational expenditure (OPEX) could be significantly reduced by better integrating the packet and the optical network. Multi-layer online topology insight can speed up troubleshooting (e.g., alarm correlation) and network operation (e.g., coordination of maintenance events), multi-layer offline topology inventory can improve service quality (e.g., detection of diversity constraint violations) and multi-layer traffic engineering can use the available network capacity more efficiently (e.g., coordination of restoration). In addition, provisioning workflows can be simplified or automated as needed across layers (e.g, to achieve bandwidth on demand, or to perform maintenance events).

ACTN framework enables this complete multi-layer and multi-vendor integration of packet and optical networks through MDSC and packet and optical PNCs.

In this document, key scenarios for Packet Optical Integration (POI) are described from the packet service layer perspective. The objective is to explain the benefit and the impact for both the packet and the optical layer, and to identify the required coordination between both layers. Precise definitions of scenarios can help with achieving a common understanding across different disciplines. The focus of the scenarios are IP/MPLS networks operated as client of optical DWDM networks. The scenarios are ordered by increasing level of integration and complexity. For each multi-layer use case, the document analyzes how to use the interfaces and data models of the ACTN architecture.

Understanding the level of standardization and the gaps will help to better assess the feasibility of integration between IP and Optical DWDM domain (and optionally OTN layer), in an end-to-end multi-vendor service provisioning perspective.

# Reference architecture and network scenario

This document analyses a number of deployment scenarios for Packet and Optical Integration (POI) in which ACTN hierarchy is deployed to control a multi‑layer and multi-domain network, with two Optical domains and two Packet domains, as shown in Figure 1:

+----------+

| MDSC |

+-----+----+

|

+-----------+-----+------+-----------+

| | | |

+----+----+ +----+----+ +----+----+ +----+----+

| P-PNC 1 | | O-PNC 1 | | O-PNC 2 | | P-PNC 2 |

+----+----+ +----+----+ +----+----+ +----+----+

| | | |

| \ / |

+-------------------+ \ / +-------------------+

CE / PE BR \ | / / BR PE \ CE

o--/---o o---\-|-------|--/---o o---\--o

\ : : / | | \ : : /

\ : PKT Domain 1 : / | | \ : PKT Domain 2 : /

+-:---------------:-+ | | +-:---------------:--+

: : | | : :

: : | | : :

+-:---------------:------+ +-------:---------------:--+

/ : : \ / : : \

/ o...............o \ / o...............o \

\ Optical Domain 1 / \ Optical Domain 2 /

\ / \ /

+------------------------+ +--------------------------+

1. – Reference Scenario

The ACTN architecture, defined in [RFC8453], is used to control this multi-domain network where each Packet PNC (P-PNC) is responsible for controlling its IP domain, which can be either an Autonomous System (AS), [RFC1930], or an IGP area within the same operator network, and each Optical PNC (O-PNC) is responsible for controlling its Optical Domain.

The routers between IP domains can be either AS Boundary Routers (ASBR) or Area Border Router (ABR): in this document the generic term Border Router (BR) is used to represent either an ASBR or a BR.

The MDSC is responsible for coordinating the whole multi‑domain multi‑layer (Packet and Optical) network. A specific standard interface (MPI) permits MDSC to interact with the different Provisioning Network Controller (O/P-PNCs).

The MPI interface presents an abstracted topology to MDSC hiding technology-specific aspects of the network and hiding topology details depending on the policy chosen regarding the level of abstraction supported. The level of abstraction can be obtained based on P-PNC and O-PNC configuration parameters (e.g. provide the potential connectivity between any PE and any BR in an MPLS-TE network).

The MDSC in Figure 1 is responsible for multi-domain and multi-layer coordination across multiple Packet and Optical domains, as well as to provide L2/L3VPN services.

From an implementation perspective, the functions associated with MDSC and described in [RFC8453] may be grouped in different ways.

1. Both the service- and network-related functions are collapsed into a single, monolithic implementation, dealing with the virtualization of the customer requests, received from the CMI, and the adaptation to the relevant network models. Such case is represented in Figure 2 of [RFC8453]
2. An implementation can choose to split the service-related and the network-related functions in different functional entities, as described in [RFC8309] and in section 4.2 of [RFC8453]. In this case, MDSC is decomposed into a top-level Service Orchestrator, interfacing the customer via the CMI, and into a Network Orchestrator interfacing at the southbound with the PNCs. The interface between the Service Orchestrator and the Network Orchestrator is not specified in [RFC8453].
3. Another implementation can choose to split the MDSC functions between an H-MDSC responsible for packet‑optical multi-layer coordination, interfacing with one Optical L-MDSC, providing multi-domain coordination between the O-PNCs and one Packet L‑MDSC, providing multi‑domain coordination betweeh the P-PNCs (see for example Figure 9 of [RFC8453].
4. Another implementation can also choose to combine the MDSC and the P-PNC functions together.

Please note that in current service provider’s network deployments, at the North Bound of the MDSC, instead of a CNC, typically there is an OSS/Orchestration layer. In this case, the MDSC would implement only the Network Orchestration functions, as described in point 2 above.

The OSS/Orchestration layer is a key part of the architecture framework for a service provider:

* to abstract (through MDSC and PNCs) the underlying transport network complexity to the Business Systems Support layer
* to coordinate NFV, Transport (e.g. IP, Optical and Microwave networks), Fixed Acess, Core and Radio domains enabling full automation of end-to-end services
* to enable catalogue-driven service provisioning from external applications (e.g. Customer Portal for Enterprise Business services) orchestrating the design and lifecycle management of these end-to-end transport connectivity services, consuming IP and/or Optical transport connectivity services upon request.

The functionality of the OSS/Orchestration layer as well as the interface toward the MDSC are usually operator-specific and outside the scope of this draft. This document assumes that the OSS/Orchestrator requests MDSC to setup L2VPN/L3VPN services through mechanisms which are outside the scope of the draft.

There are two main cases when MDSC coordination of underlying PNCs in POI context is initiated:

* Initiated by a request from the OSS/Orchestration layer to setup L2VPN/L3VPN services that requires multi-layer/multi-domain coordination.
* Initiated by the MDSC itself to perform multi-layer/multi-domain optimizations and/or maintenance works, beyond discovery (e.g. rerouting LSPs with their associated services when putting a resource, like a fibre, in maintenance mode during a maintenance window). Different to service fulfillment, the workflows then are not related at all to a service provisioning request being received from the OSS/Orchestration layer.

Above two MDSC workflow cases are in the scope of this draft or in future versions.

In the network scenario of Figure 1, it is assumed that:

* The domain boundaries between the IP and Optical domains are congruent. In other words, one Optical domain supports connectivity between Routers in one and only one Packet Domain;
* Inter-domain links exist only between Packet domains (i.e., between ASBR routers) and between Packet and Optical domains (i.e., between routers and Optical NEs). In other words, there are no inter-domain links between Optical domains;
* The interfaces between the Routers and the Optical NEs are “Ethernet” physical interfaces;
* The interfaces between the Border Routers (BRs) are “Ethernet” physical interfaces.

This version of the document assumes that the IP Link supported by the Optical netork are always intra-AS (PE-BR, PE-P or P-P) and that the BRs are co-located and connected by an IP Link supported by an Ethernet physical link.

The possibility to setup inter-AS IP Links (e.g., BR-BR or PE-PE), supported by Optical network, is for further study.

Therefore, if inter-domain links between the Optical domains exist, they would be used to support multi-domain Optical services, which are outside the scope of this document.

The Optical NEs within the optical domains can be ROADMs or OTN switches, with or without a ROADM.

## Generic Assumptions

This section describes general assumptions which are applicable at all the MPI interfaces, between each PNC (Optical or Packet) and the MDSC, and also to all the scenarios discussed in this document.

The data models used on these interfaces are assumed to use the YANG 1.1 Data Modeling Language, as defined in [RFC7950].

The RESTCONF protocol, as defined in [RFC8040], using the JSON representation, defined in [RFC7951], is assumed to be used at these interfaces. Extensions to RESTCONF, as defined in [RFC8527], to be compliant with Network Management Datastore Architecture (NMDA) defined in [RFC8342], are assumed to be used as well at these MPI interfaces and also at CMI interfaces.

As required in [RFC8040], the "ietf-yang-library" YANG module defined in [RFC8525] is used to allow the MDSC to discover the set of YANG modules supported by each PNC at its MPI.

## L2/L3VPN Service Request in North Bound of MDSC

As explained in section 2, the OSS/Orchestration layer can request the MDSC to setup of L2/L3VPN services (with or without TE requirements).

Although the interface between the OSS/Orchestration layer is usually operator-specific, Figure 2 shows an example of a possible control flow between the OSS/Orchestration layer and the MDSC to instantiate L2/L3VPN services, using the YANG models under definition in [VN], [L2NM], [L3NM] and [TSM].

+-------------------------------------------+

| |

| OSS/Orchestration layer |

| |

+-----------------------+-------------------+

|

1.VN 2. L2/L3NM & | ^

| TSM | |

| | | |

| | | |

v v | 3. Update VN

|

+-----------------------+-------------------+

| |

| MDSC |

| |

+-------------------------------------------+

1. Service Request Process

* The VN YANG model [VN], whose primary focus is the CMI, can also be used to provide VN Service configuration from a orchestrated connectivity service point of view, when the L2/L3VPN service has TE requirements. This model is not used to setup L2/L3VPN service with no TE requirements.
  + It provides the profile of VN in terms of VN members, each of which corresponds to an edge-to-edge link between customer end-points (VNAPs). It also provides the mappings between the VNAPs with the LTPs and between the connectivity matrix with the VN member from which the associated traffic matrix (e.g., bandwidth, latency, protection level, etc.) of VN member is expressed (i.e., via the TE-topology’s connectivity matrix).
  + The model also provides VN-level preference information (e.g., VN member diversity) and VN-level admin-status and operational-status.
* The L2NM YANG model [L2NM], whose primary focus is the MPI, can also be used to provideL2VPN service configuration and site information, from a orchestrated connectivity service point of view.
* The L3NM YANG model [L3NM], whose primary focus is the MPI, can also be used to provide all L3VPN service configuration and site information, from a orchestrated connectivity service point of view.
* The TE & Service Mapping YANG model [TSM] provides TE-service mapping as well as site mapping.
  + TE-service mapping provides the mapping between a L2/L3VPN instance and the corresponding VN instances.
  + The TE-service mapping also provides the service mapping requirement type as to how each L2/L3VPN/VN instance is created with respect to the underlay TE tunnels (e.g., whether they require a new and isolated set of TE underlay tunnels or not). See Section 2.3 for detailed discussion on the mapping requirement types.
  + Site mapping provides the site reference information across L2/L3VPN Site ID, VN Access Point ID, and the LTP of the access link.

## Service and Network Orchestration

From a functional standpoint, MDSC represented in Figure 2 interfaces with the OSS/Orchestration layer and decouples L2/L3VPN service configuration functions from network configuration functions. Therfore in this document the MDSC performs the functions of the Network Orchestrator, as defined in [RFC 8309].

One of the important MDSC functions is to identify which TE Tunnels should carry the L2/L3VPN traffic (e.g., from TE & Service Mapping configuration) and to relay this information to the P-PNCs, to ensure the PEs’ forwarding tables (e.g., VRF) are properly populated, according to the TE binding requirement for the L2/L3VPN.

TE binding requirement types [TSM] are:

1. Hard Isolation with deterministic latency: The L2/L3VPN service requires a set of dedicated TE Tunnels providing deterministic latency performances and that cannot be not shared with other services, nor compete for bandwidth with other Tunnels.
2. Hard Isolation: This is similar to the above case without deterministic latency requirements.
3. Soft Isolation: The L2/L3VPN service requires a set of dedicated MPLS-TE tunnels which cannot be shared with other services, but which could compete for bandwidth with other Tunnels.
4. Sharing: The L2/L3VPN service allows sharing the MPLS-TE Tunnels supporting it with other services.

For the first three types, there could be additional TE binding requirements with respect to different VN members of the same VN (on how different VN members, belonging to the same VN, can share or not network resources). For the first two cases, VN members can be hard-isolated, soft-isolated, or shared. For the third case, VN members can be soft-isolated or shared.

In order to fulfill the the L2/L3VPN end-to-ende TE requirements, including the TE binding rquirements, the MDSC needs to perform multi-layer/multi-domain path computation to select the BRs, the intra-domain MPS-TE Tunnels and the intra-domain Optical Tunnels.

Depending on the knowledge that MDSC has of the topology and configuration of the underlying network domains, three models for performing path computation are possible:

1. Summarization: MDSC has an abstracted TE topology view of all of the underlying domains, both packet and optical. MDSC does not have enough TE topology information to perform multi‑layer/multi‑domain path computation. Therefore MDSC delegates the P-PNCs and O-PNCs to perform a local path computation within their controlled domains and it uses the information returned by the P-PNCs and O-PNCs to compute the optimal multi-domain/multi-layer path.   
   This model presents an issue to P-PNC, which does not have the capability of performing a single-domain/multi-layer path computation (that is, P-PNC does not have any possibility to retrieve the topology/configuration information from the optical controller). A possible solution could be to include a CNC function in the P‑PNC to request the MDSC multi-domain Optical path computation, as shown in Figure 10 of [RFC8453].
2. Partial summarization: MDSC has full visibility of the TE topology of the packet network domains and an abstracted view of the TE topology of the optical network domains.   
   MDSC then has only the capability of performing multi-domain/single-layer path computation for the packet layer (the path can be computed optimally for the two packet domains). Therefore MDSC still needs to delegate the O-PNCs to perform local path computation within their respective domains and it uses the information received by the O‑PNCs, together with its TE topology view of the multi‑domain packet layer, to perform multi‑layer/multi‑domain path computation.  
   The role of P-PNC is minimized, i.e. is limited to management.
3. Full knowledge: MDSC has the complete and enough detailed view of the TE topology of all the network domains (both optical and packet). In such case MDSC has all the information needed to perform multi-domain/multi-layer path computation, without relying on PNCs.  
   This model may present, as a potential drawback, scalability issues and, as discussed in section 2.2. of [PATH-COMPUTE], performing path computation for optical networks in the MDSC is quite challenging because the optimal paths depend also on vendor‑specific optical attributes (which may be different in the two domains if they are provided by different vendors).

The current version of this draft assumes that MDSC supports model #2 (Partial summarization).

*[Note: check with opeerators for some references on real deployment]*

### Hard Isolation

For example, when “Hard Isolation with or w/o deterministic latency” TE binding requirement is applied for a L2/L3VPN, new Optical by‑pass Tunnels needs to be setup between PEs and BRs.

The MDSC needs to identify the set of IP/MPLS domains and their BRs. This requires the MDSC to request each O‑PNC to compute the intra‑domain optical paths between each PEs/BRs pairs.

When requesting optical path computation to the O-PNC, the MDSC needs to take into account the inter-layer peering points, such as the interconnections between the PE/BR nodes and the edge Optical nodes (e.g., using the inter-layer lock or the transitional link information, defined in [RFC8795]).

When the optimal multi‑layer/multi-domain path has been computed, the MDSC requests each O-PNC to setup the selected Optical Tunnels and P‑PNC to setup the intra‑domain MPLS‑TE Tunnels, over the selected Optical Tunnels. MDSC also properly configures its BGP speakers and PE/BR forwarding tables to ensure that the VPN traffic is properly forwarded.

### Shared Tunnel Selection

In case of shared tunnel selection, the MDSC needs to check if there is multi‑domain path which can support the L2/L3VPN end-to-end TE service requirements (e.g., bandwidth, latency, etc.) using existing intra-domain MPLS-TE tunnels.

If such a path is found, the MDSC selects the optical path from the candidate pool and request each P‑PNC to setup the L2/L3VPN service using the selected intra­‑domain MPLS‑TE tunnel, between PE/BR nodes.

Otherwise, the MDSC should detect if the multi‑domain path can be setup using existing intra‑domain MPLS-TE tunnels with modifications (e.g., increasing the tunnel bandwidth) or setting up new intra-domain MPLS‑TE tunnel(s).

The modification of an existing MPLS‑TE Tunnel as well as the setup of a new MPLS‑TE Tunnel may also require multi‑layer coordination e.g., in case the available bandwidth of underlying Optical Tunnels is not sufficient. Based on multi‑domain/multi‑layer path computation, the MDSC can decide for example to modify the bandwidth of an existing Optical Tunnel (e.g., ODUflex bandwidth increase) or to setup new Optical Tunnels to be used as additional LAG members of an existing IP Link or as new IP Links to re-route the MPLS‑TE Tunnel.

In all the cases, the labels used by the end-to-end tunnel are distributed in the PE and BR nodes by BGP. The MDSC is responsible to configure the BGP speakeers in each P‑PNC, if needed.

## IP/MPLS Domain Controller and NE Functions

IP/MPLS networks are assumed to have multiple domains, where each domain, corresponding to either an IGP area or an Autonomous System (AS) within the same operator network, is controlled by an IP/MPLS domain controller (P‑PNC).

Among the functions of the P‑PNC, there are the setup or modification of the intra‑domain MPLS-TE Tunnels, between PEs and BRs, and the configuration of the VPN services, such as the VRF in the PE nodes, as shown in Figure 3:

+------------------+ +------------------+

| | | |

| P‑PNC1 | | P‑PNC2 |

| | | |

+--|-----------|---+ +--|-----------|---+

| 1.Tunnel | 2.VPN | 1.Tunnel | 2.VPN

| Config | Provisioning | Config | Provisioning

V V V V

+---------------------+ +---------------------+

CE / PE tunnel 1 BR\ / BR tunnel 2 PE \ CE

o--/---o..................o--\-----/--o..................o---\--o

\ / \ /

\ Domain 1 / \ Domain 2 /

+---------------------+ +---------------------+

End-to-end tunnel

<------------------------------------------------->

1. IP/MPLS Domain Controller & NE Functions

It is assumed that BGP is running in the inter-domain IP/MPLS networks for L2/L3VPN and that the P‑PNC controller is also responsible for configuring the BGP speakers within its control domain, if necessary.

The BGP would be responsible for the label distribution of the end‑to‑end tunnel on PE and BR nodes. The MDSC is responsible for the selection of the BRs and of the intra-domain MPLS‑TE Tunnels between PE/BR nodes.

If new MPLS‑TE Tunnels are needed or mofications (e.g., bandwidth ingrease) to existing MPLS\_TE Tunnels are needed, as outlined in section 2.3, the MDSC would request their setup or modifications to the P‑PNCs (step 1 in Figure 3). Then the MDSC would request the P‑PNC to configure the VPN, including the selection of the intra‑domain TE Tunnel (step 2 in Figure 3).

The P‑PNC should configure, using mechanisms outside the scope of this document, the ingress PE forwarding table, e.g., the VRF, to forward the VPN traffic, received from the CE, with the following three labels:

* VPN label: assigned by the egress PE and distributed by BGP;
* end‑to‑end LSP label: assigned by the egress BR, selected by the MDSC, and distributed by BGP;
* MPLS-TE tunnel label, assigned by the next hop P node of the tunnel selected by the MDSC and distributed by mechanism internal to the IP/MPLS domain (e.g., RSVP-TE).

## Optical Domain Controller and NE Functions

Optical network provides the underlay connectivity services to IP/MPLS networks. The coordination of Packet/Optical multi-layer is done by the MDSC, as shown in Figure 1.

The O‑PNC is responsible to:

* provide to the MDSC an abstract TE topology view of its underlying optical network resources;
* perform single‑domain local path computation, when requested by the MDSC;
* perform Optical Tunnel setup, when requested by the MDSC.

The mechanisms used by O‑PNC to perform intra‑domain topology discovery and path setup are usually vendor‑speicific and outside the scope of this document.

Depending on the type of optical network, TE topology abstraction, path compution and path setup can be single‑single (either OTN or WDM) or multi-layer OTN/WDM. In the latter case, the multi-layer coordination between the OTN and WDM layers is performed by the O‑PNC.

# Multi-layer and multi-domain services scenarios

Multi-layer and multi-domain scenarios, based on reference network described in section 2 , and very relevant for Service Providers, are described in the next sections. For each scenario existing IETF protocols and data models are identified with particular focus on the MPI in the ACTN architecture. Non ACTN IETF data models required for L2/L3VPN service provisioning between MDSC and IP PNCs are also identified.

## Scenario 1: network and service topology discovery

In this scenario, the MSDC needs to discover through the underlying PNCs, the network topology, at both WDM and IP layers, in terms of nodes (NEs) and links, including inter AS domain links as well as cross-layer links but also in terms of tunnels (MPLS or SR paths in IP layer and OCh and optionally ODUk tunnels in optical layer).MDSC discovers also the IP/MPLS transport services (L2VPN/L3VPN) deployed, both intra-domain and inter-domain wise.

Each PNC provides to the MDSC an abstracted or full topology view of the WDM or the IP topology of the domain it controls. This topology can be abstracted in the sense that some detailed NE information is hidden at the MPI, and all or some of the NEs and related physical links are exposed as abstract nodes and logical (virtual) links, depending on the level of abstraction the user requires. This information is key to understand both the inter-AS domain links (seen by each controller as UNI interfaces but as I-NNI interfaces by the MDSC) as well as the cross-layer mapping between IP and WDM layer.

The MDSC also maintains an up-to-date network database of both IP and WDM layers (and optionally OTN layer) through the use of IETF notifications through MPI with the PNCs when any topology change occurs. It should be possible also to correlate information coming from IP and WDM layers (e.g.: which port, lambda/OTSi, direction is used by a specific IP service on the WDM equipment)

In particular, For the cross-layer links it is key for MDSC to be able to correlate automatically the information from the PNC network databases about the physical ports from the routers (single link or bundle links for LAG) to client ports in the ROADM.

It should be possible at MDSC level to easily correlate WDM and IP layers alarms to speed-up troubleshooting

Alarms and event notifications are required between MDSC and PNCs so that any network changes are reported almost in real-time to the MDSC (e.g. NE or link failure, MPLS tunnel switched from main to backup path etc.). As specified in [RFC7923] MDSC must be able to subscribe to specific objects from PNC YANG datastores for notifications.

### Common YANG models used at MPIs

Both Optical and Packet PNCs use the following common topology YANG models at the MPI to report their abstract topologies:

* The Base Network Model, defined in the “ietf-network” YANG module of [RFC8345]
* The Base Network Topology Model, defined in the “ietf-network-topology” YANG module of [RFC8345], which augments the Base Network Model
* The TE Topology Model, defined in the “ietf-te-topology” YANG module of [TE-TOPO], which augments the Base Network Topology Model

These common YANG models are generic and augmented by technology-specific YANG modules as described in the following sections.

Both Optical and Packet PNCs must use the following common notifications YANG models at the MPI so that any network changes can be reported almost in real-time to MDSC by the PNCs:

* Dynamic Subscription to YANG Events and Datastores over RESTCONF as defined in [RFC8650]
* Subscription to YANG Notifications for Datastores updates as defined in [RFC8641]

PNCs and MDSCs must be compliant with subscription requirements as stated in [RFC7923].

### Required YANG models at the optical MPIs

The Optical PNC also uses at least the following technology-specific topology YANG models, providing WDM and Ethernet technology-specific augmentations of the generic TE Topology Model:

* The WSON Topology Model, defined in the “ietf-wson-topology” YANG modules of [WSON-TOPO], or the Flexi‑grid Topology Model, defined in the “ietf-flexi-grid-topology” YANG module of [Flexi‑TOPO].
* Optionally the OTN Topology Model, defined in the “ietf-otn-topology” YANG module of the draft draft-ietf-ccamp-otn-topo-yang-10 [OTN-TOPO]
* The Ethernet Topology Model, defined in the “ietf-eth-te-topology” YANG module of [CLIENT-TOPO]
* Optionally when OTN layer is used, the network data model for L1 OTN services (e.g. an Ethernet transparent service) as defined in “ietf-trans-client-service” YANG module of draft-ietf-ccamp-client-signal-yang [CLIENT-SIGNAL]

The WSON Topology Model or, alternatively, the Flexi‑grid Topology model is used to report the DWDM network topology (e.g., ROADMs and links) depending on whether the DWDM optical network is based on fixed grid or flexible-grid.

The Ethernet Topology is used to report the access links between the IP routers and the edge ROADMs.

### Required YANG models at the Packet MPIs

The Packet PNC also uses at least the following technology-specific topology YANG models, providing IP and Ethernet technology-specific augmentations of the generic Topology Models described in section 3.1.1. :

* The L3 Topology Model, defined in the “ietf‑l3‑unicast‑topology” YANG modules of [RFC8346], which augments the Base Network Topology Model
* The L3 specific data model including extended TE attributes (e.g. performance derived metrics like latency), defined in “ietf-l3-te-topology” and in “ietf-te-topology-packet” in draft-ietf-teas-l3-te-topo [L3-TE-TOPO]
* The Ethernet Topology Model, defined in the “ietf-eth-te-topology” YANG module of [CLIENT-TOPO], which augments the TE Topology Model

The Ethernet Topology Model is used to report the access links between the IP routers and the edge ROADMs as well as the inter‑domain links between ASBRs, while the L3 Topology Model is used to report the IP network topology (e.g., IP routers and links).

* The User Network Interface (UNI) Topology Model, being defined in the “ietf-uni-topology” module of the draft-ogondio-opsawg-uni-topology [UNI-TOPO] which augment “ietf-network” module defined in [RFC8345] adding service attachment points to the nodes to which L2VPN/L3VPN IP/MPLS services can be attached.
* L3VPN network data model defined in “ietf-l3vpn-ntw” module of draft-ietf-opsawg-l3sm-l3nm [L3NM] used for non-ACTN MPI for L3VPN service provisioning
* L2VPN network data model defined in “ietf-l2vpn-ntw” module of draft-ietf-barguil-opsawg-l2sm-l2nm [L2NM] used for non-ACTN MPI for L2VPN service provisioning

### Inter-domain link discovery

In the reference network of Figure 1, there are two types of inter‑domain links:

* Links between two IP domains (ASes)
* Links between an IP router and a ROADM

Both types of links are Ethernet physical links.

The inter-domain link information is reported to the MDSC by the two adjacent PNCs, controlling the two ends of the inter-domain link.

The MDSC can understand how to merge these inter‑domain links together using the plug-id attribute defined in the TE Topology Model [TE‑TOPO], as described in as described in section 4.3 of [TE-TOPO].

A more detailed description of how the plug-id can be used to discover inter-domain link is also provided in section 5.1.4 of [TNBI].

Both types of inter‑domain links are discovered using the plug‑id attributes reported in the Ethernet Topologies exposed by the two adjacent PNCs. The MDSC can also discover an inter‑domain IP link/adjacency between the two IP LTPs, reported in the IP Topologies exposed by the two adjacent P‑PNCs, supported by the two ETH LTPs of an Ethernet Link discovered between these two P‑PNCs.

Two options are possible to discover these inter‑domain links:

1. Static configuration
2. LLDP [IEEE 802.1AB] automatic discovery

Since the static configuration requires an administrative burden to configure network-wide unique identifiers, the automatic discovery solution based on LLDP is preferable when LLDP is supported.

As outlined in [TNBI], the encoding of the plug-id namespace as well as of the LLDP information within the plug-id value is implementation specific and needs to be consistent across all the PNCs.

## L2VPN/L3VPN establishment

To be added

***[Editor’s Note]*** *What mechanism would convey on the interface to the IP/MPLS domain controllers as well as on the SBI (between IP/MPLS domain controllers and IP/MPLS PE routers) the TE binding policy dynamically for the L3VPN? Typically, VRF is the function of the device that participate MP-BGP in MPLS VPN. With current MP-BGP implementation in MPLS VPN, the VRF’s BGP next hop is the destination PE and the mapping to a tunnel (either an LDP or a BGP tunnel) toward the destination PE is done by automatically without any configuration. It is to be determined the impact on the PE VRF operation when the tunnel is an optical bypass tunnel which does not participate either LDP or BGP.*

***New text to answer the yellow part:***

The MDSC Network-related function will then coordinate with the PNCs involved in the process to provide the provisioning information through ACTN MDSC to PNC (MPI) interface. The relevant data models used at the MPI may be in the form of L3NM, L2NM or others and are exchanged through MPI API calls. Through this process MDSC Network-related functions provide the configuration information to realize a VPN service to PNCs. For example, this process will inform PNCs on what PE routers compose a L3VPN, the topology requested, the VPN attributes, etc.

At the end of the process PNCs will deliver the actual configuration to the devices (either physical or virtual), through the ACTN Southbound Interface (SBI). In this case the configuration policies may be exchanged using a Netconf session delivering configuration commands associated to device-specific data models (e.g. BGP[], QOS [], etc.).

Having the topology information of the network domains under their control, PNCs will deliver all the information necessary to create, update, optimize or delete the tunnels connecting the PE nodes as requested by the VPN instantiation.

# Security Considerations

Several security considerations have been identified and will be discussed in future versions of this document.

# Operational Considerations

Telemetry data, such as the collection of lower-layer networking health and consideration of network and service performance from POI domain controllers, may be required. These requirements and capabilities will be discussed in future versions of this document.

# IANA Considerations

This document requires no IANA actions.

# References

## Normative References

[RFC7950] Bjorklund, M. et al., "The YANG 1.1 Data Modeling Language", RFC 7950, August 2016.

[RFC7951] Lhotka, L., "JSON Encoding of Data Modeled with YANG", RFC 7951, August 2016.

[RFC8040] Bierman, A. et al., "RESTCONF Protocol", RFC 8040, January 2017.

[RFC8345] Clemm, A., Medved, J. et al., “A Yang Data Model for Network Topologies”, RFC8345, March 2018.

[RFC8346] Clemm, A. et al., “A YANG Data Model for Layer 3 Topologies”, RFC8346, March 2018.

[RFC8453] Ceccarelli, D., Lee, Y. et al., "Framework for Abstraction and Control of TE Networks (ACTN)", RFC8453, August 2018.

[RFC8525] Bierman, A. et al., "YANG Library", RFC 8525, March 2019.

[IEEE 802.1AB] IEEE 802.1AB-2016, "IEEE Standard for Local and metropolitan area networks - Station and Media Access Control Connectivity Discovery", March 2016.

[TE-TOPO] Liu, X. et al., "YANG Data Model for TE Topologies", draft-ietf-teas-yang-te-topo, work in progress.

[WSON-TOPO] Lee, Y. et al., " A YANG Data Model for WSON (Wavelength Switched Optical Networks)", draft-ietf-ccamp-wson-yang, work in progress.

[Flexi‑TOPO] Lopez de Vergara, J. E. et al., "YANG data model for Flexi-Grid Optical Networks", draft-ietf-ccamp-flexigrid-yang, work in progress.

[CLIENT-TOPO] Zheng, H. et al., "A YANG Data Model for Client-layer Topology", draft-zheng-ccamp-client-topo-yang, work in progress.

[L3-TE-TOPO] Liu, X. et al., "YANG Data Model for Layer 3 TE Topologies", draft-ietf-teas-yang-l3-te-topo, work in progress.

[TE-TUNNEL] Saad, T. et al., "A YANG Data Model for Traffic Engineering Tunnels and Interfaces", draft-ietf-teas-yang-te, work in progress.

[WSON‑TUNNEL] Lee, Y. et al., "A Yang Data Model for WSON Tunnel", draft-ietf-ccamp-wson-tunnel-model, work in progress.

[Flexi‑MC] Lopez de Vergara, J. E. et al., "YANG data model for Flexi-Grid media-channels", draft-ietf-ccamp-flexigrid-media-channel-yang, work in progress.

[CLIENT-SIGNAL] Zheng, H. et al., "A YANG Data Model for Transport Network Client Signals", draft-ietf-ccamp-client-signal-yang, work in progress.

## Informative References

[RFC1930] J. Hawkinson, T. Bates, “Guideline for creation, selection, and registration of an Autonomous System (AS)”, RFC 1930, March 1996.

[RFC4364] E. Rosen and Y. Rekhter, “BGP/MPLS IP Virtual Private Networks (VPNs)”, RFC 4364, February 2006.

[RFC4761] K. Kompella, Ed., Y. Rekhter, Ed., “Virtual Private LAN Service (VPLS) Using BGP for Auto-Discovery and Signaling”, RFC 4761, January 2007.

[RFC6074] E. Rosen, B. Davie, V. Radoaca, and W. Luo, “Provisioning, Auto-Discovery, and Signaling in Layer 2 Virtual Private Networks (L2VPNs)”, RFC 6074, January 2011.

[RFC6624] K. Kompella, B. Kothari, and R. Cherukuri, “Layer 2 Virtual Private Networks Using BGP for Auto-Discovery and Signaling”, RFC 6624, May 2012.

[RFC7209] A. Sajassi, R. Aggarwal, J. Uttaro, N. Bitar, W. Henderickx, and A. Isaac, “Requirements for Ethernet VPN (EVPN)”, RFC 7209, May 2014.

[RFC7432] A. Sajassi, Ed., et al., “BGP MPLS-Based Ethernet VPN”, RFC 7432, February 2015.

[RFC7436] H. Shah, E. Rosen, F. Le Faucheur, and G. Heron, “IP-Only LAN Service (IPLS)”, RFC 7436, January 2015.

[RFC8214] S. Boutros, A. Sajassi, S. Salam, J. Drake, and J. Rabadan, “Virtual Private Wire Service Support in Ethernet VPN”, RFC 8214, August 2017.

[RFC8299] Q. Wu, S. Litkowski, L. Tomotaki, and K. Ogaki, “YANG Data Model for L3VPN Service Delivery”, RFC 8299, January 2018.

[RFC8309] Q. Wu, W. Liu, and A. Farrel, “Service Model Explained”, RFC 8309, January 2018.

[RFC8466] G. Fioccola, ed., “A YANG Data Model for Layer 2 Virtual Private Network (L2VPN) Service Delivery”, RFC8466, October 2018.

[TNBI] Busi, I., Daniel, K. et al., "Transport Northbound Interface Applicability Statement", draft-ietf-ccamp-transport-nbi-app-statement, work in progress.

[VN] Y. Lee, et al., “A Yang Data Model for ACTN VN Operation”, draft-ietf-teas-actn-vn-yang, work in progress.

[L2NM] S. Barguil, et al., “A Layer 2 VPN Network YANG Model”, draft-ietf-opsawg-l2nm, work in progress.

[L3NM] S. Barguil, et al., “A Layer 3 VPN Network YANG Model”, draft-ietf-opsawg-l3sm-l3nm, work in progress.

[TSM] Y. Lee, et al., “Traffic Engineering and Service Mapping Yang Model”, draft-ietf-teas-te-service-mapping-yang, work in progress.

[ACTN-PM] Y. Lee, et al., “YANG models for VN & TE Performance Monitoring Telemetry and Scaling Intent Autonomics”, draft-lee-teas-actn-pm-telemetry-autonomics, work in progress.

[BGP-L3VPN] D. Jain, et al. “Yang Data Model for BGP/MPLS L3 VPNs”, draft-ietf-bess-l3vpn-yang, work in progress.

# Acknowledgments

This document was prepared using 2-Word-v2.0.template.dot.

Some of this analysis work was supported in part by the European Commission funded H2020-ICT-2016-2 METRO-HAUL project (G.A. 761727).

1. Multi-layer and multi-domain resiliency
   1. Maintenance Window

To be added

* 1. Router port failure

To be added

Authors’ Addresses

Fabio Peruzzini

TIM

Email: [fabio.peruzzini@telecomitalia.it](mailto:fabio.peruzzini@telecomitalia.it)

Jean-Francois Bouquier  
Vodafone

Email: [jeff.bouquier@vodafone.com](mailto:jeff.bouquier@vodafone.com)

Italo Busi  
Huawei

Email: [Italo.busi@huawei.com](mailto:Italo.busi@huawei.com)

Daniel King  
Old Dog Consulting

Email: [daniel@olddog.co.uk](mailto:daniel@olddog.co.uk)

Daniele Ceccarelli  
Ericsson

Email: [daniele.ceccarelli@ericsson.com](mailto:daniele.ceccarelli@ericsson.com)

Sergio Belotti  
Nokia

Email: [sergio.belotti@nokia.com](mailto:sergio.belotti@nokia.com)

Gabriele Galimberti  
Cisco

Email: [ggalimbe@cisco.com](mailto:ggalimbe@cisco.com)

Zheng Yanlei  
China Unicom

Email: [zhengyanlei@chinaunicom.cn](mailto:zhengyanlei@chinaunicom.cn)

Anton Snitser  
Sedona

Email: [antons@sedonasys.com](mailto:antons@sedonasys.com)

Washington Costa Pereira Correia  
TIM Brasil

Email: [wcorreia@timbrasil.com.br](mailto:wcorreia@timbrasil.com.br)

Michael Scharf  
Hochschule Esslingen - University of Applied Sciences

Email: [michael.scharf@hs-esslingen.de](mailto:michael.scharf@hs-esslingen.de)

Young Lee  
Sung Kyun Kwan University

Email: [younglee.tx@gmail.com](mailto:younglee.tx@gmail.com)

Jeff Tantsura  
Apstra

Email: [jefftant.ietf@gmail.com](mailto:jefftant.ietf@gmail.com)